# Print guide — byitl_di01_drip_irrigation

One card per printed part — how it lands on the bed, its size, and whether it needs supports.

| Part | Size (mm) | Weight | Print orientation (rx,ry,rz) | Supports |
| --- | --- | --- | --- | --- |
| enclosure_base | 186×130×43 | ~100 g | 0,0,0 | support-free |
| enclosure_lid | 186×130×7 | ~36 g | 0,0,0 | support-free |
| manifold | 90×38×38 | ~37 g | 0,0,0 | support-free |
| pump_strap | 42×42×6 | ~5 g | 0,0,0 | support-free |
| battery_strap | 98×30×6 | ~9 g | 0,0,0 | support-free |
| solar_stake | 120×100×125 | ~79 g | 0,90,0 | 1144 mm² overhang |
| rim_clamp | 32×24×43 | ~4 g | 0,0,0 | support-free |

## Parts
### enclosure_base

![enclosure_base](print-cards/enclosure_base.png)

### enclosure_lid

![enclosure_lid](print-cards/enclosure_lid.png)

### manifold

![manifold](print-cards/manifold.png)

### pump_strap

![pump_strap](print-cards/pump_strap.png)

### battery_strap

![battery_strap](print-cards/battery_strap.png)

### solar_stake

![solar_stake](print-cards/solar_stake.png)

### rim_clamp

![rim_clamp](print-cards/rim_clamp.png)

