# Print guide — byitl_hp01_hydroponic_plant_pot

One card per printed part — how it lands on the bed, its size, and whether it needs supports.

| Part | Size (mm) | Weight | Print orientation (rx,ry,rz) | Supports |
| --- | --- | --- | --- | --- |
| reservoir_body | 160×136×170 | ~167 g | 0,0,0 | support-free |
| lid | 167×137×20 | ~64 g | 0,90,0 | 2681 mm² overhang |
| electronics_tower | 120×62×150 | ~107 g | 0,0,0 | 950 mm² overhang |
| tower_cover | 120×62×10 | ~22 g | 180,0,0 | support-free |
| grow_ring | 168×138×34 | ~150 g | 180,0,0 | support-free |
| window_bezel | 66×6×125 | ~15 g | 0,0,0 | support-free |
| net_cup | 84×84×75 | ~19 g | 0,0,0 | support-free |

## Parts
### reservoir_body

![reservoir_body](print-cards/reservoir_body.png)

### lid

![lid](print-cards/lid.png)

### electronics_tower

![electronics_tower](print-cards/electronics_tower.png)

### tower_cover

![tower_cover](print-cards/tower_cover.png)

### grow_ring

![grow_ring](print-cards/grow_ring.png)

### window_bezel

![window_bezel](print-cards/window_bezel.png)

### net_cup

![net_cup](print-cards/net_cup.png)

