# Assembly guide — byitl_hp01_hydroponic_plant_pot

Each step adds one part (shown highlighted). Hardware is listed per step.

## Step 1 — attach `lid`
Fasten with **1× Lid seat (skirt over rim, no hardware)**.

![step 1](assembly-steps/step-01.png)

## Step 2 — attach `electronics_tower`
Fasten with **4× M3x10 self-tapping**.

![step 2](assembly-steps/step-02.png)

## Step 3 — attach `tower_cover`
Fasten with **4× M3x12 self-tapping**.

![step 3](assembly-steps/step-03.png)

## Step 4 — attach `light_sensor`
Fasten with **2× M2x8 self-tapping**.

![step 4](assembly-steps/step-04.png)

## Step 5 — attach `mcu_feather`
Fasten with **4× M2x8 self-tapping**.

![step 5](assembly-steps/step-05.png)

## Step 6 — attach `mosfet_driver`
Fasten with **2× M2x8 self-tapping**.

![step 6](assembly-steps/step-06.png)

## Step 7 — attach `grow_ring`
Fasten with **4× Press-fit locating pegs (no hardware)**.

![step 7](assembly-steps/step-07.png)

## Step 8 — attach `window_bezel`
Fasten with **4× M3x12 self-tapping**.

![step 8](assembly-steps/step-08.png)

## Step 9 — attach `net_cup`
Fasten with **1× Net-cup lip seat (no hardware)**.

![step 9](assembly-steps/step-09.png)

## Step 10 — attach `ph_probe`
Fasten with **1× Probe well seat (BNC shoulder on catch rim)**.

![step 10](assembly-steps/step-10.png)

