# Print guide — byitl_sp01_smart_plant_pot

One card per printed part — how it lands on the bed, its size, and whether it needs supports.

| Part | Size (mm) | Weight | Print orientation (rx,ry,rz) | Supports |
| --- | --- | --- | --- | --- |
| pot_body | 209×186×234 | ~363 g | 0,0,90 | 772 mm² overhang |
| saucer | 210×210×15 | ~88 g | 0,0,0 | support-free |
| enclosure_base | 234×110×105 | ~179 g | 0,0,0 | support-free |
| enclosure_lid | 234×110×3 | ~37 g | 0,0,0 | support-free |
| reservoir_tank | 141×88×94 | ~72 g | 0,0,0 | support-free |
| pump_strap | 11×48×6 | ~1 g | 0,0,0 | support-free |
| fill_cap | 42×42×10 | ~5 g | 0,0,0 | support-free |

## Parts
### pot_body

![pot_body](print-cards/pot_body.png)

### saucer

![saucer](print-cards/saucer.png)

### enclosure_base

![enclosure_base](print-cards/enclosure_base.png)

### enclosure_lid

![enclosure_lid](print-cards/enclosure_lid.png)

### reservoir_tank

![reservoir_tank](print-cards/reservoir_tank.png)

### pump_strap

![pump_strap](print-cards/pump_strap.png)

### fill_cap

![fill_cap](print-cards/fill_cap.png)

